|  |
| --- |
| **Standard Unit Specifications** |
| ● Jamb: Primed Pine, 5/4” x Various |
| ● Trim: WM180 Brick Moulding, 1-1/4” x 2” |
| ● Sill Threshold: Fixed Aluminum, Thermal Break |
| ● Bore: 2-1/8” Face, 2-3/8” Backset |
| ● Hinges: 4” Zinc Dichromate (3/door) |
| ● Weatherstrip: Foam Compression |
| ● Sweep: 4 Fin Vinyl |
| ● Handing: Must Specify Left or Right |

|  |
| --- |
| **Door Handing Guide** |
| **interior_door_handings.gif** |
| ● When the door opens toward you and the knob is on the LEFT it is a LEFT HAND opening |
| ● When the door opens toward you and the knob is on the RIGHT it is a RIGHT HAND opening |
| **This description of handing applies to all the door units we build, both inswing and outswing.** |

|  |  |  |
| --- | --- | --- |
| **Unit Pricing** | | |
| **Base** | Price of standard unit (frame only) | Page A2 |
| **+** | Add cost of door(s) | Section B |
| **+** | Add cost of sidelight(s) | Page A4 |
| **+** | Add cost of transom sash & frame | Page A5 |
| **+** | Add cost of multipoint lock | Page A6 |
| **+/-** | Adjust price for options | Page A3 |
| **=** | **Total Unit List Price** | |

EDU/DEDU

**Standard Door Units - Frame Only - Add Components**

***See Page A1 for Standard Specifications, Handing, and Unit Pricing information***

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | **Frame** | | | | |
| lineart-door-single.gif | **Style A – Single** | | | FJ | S | 514S | 6916S | 6916FJ |
| **Door Size** | | **Rough Opening** | **4-9/16”**  **Fingerjoint** | **4-9/16”**  **Solid** | **5-1/4”**  **Solid** | **6-9/16”**  **Solid** | **6-9/16”**  **Fingerjoint** |
| 2’8” x 6’8” | | 2’10-5/8” x 6’11” | 155.80 | 237.00 | 287.80 | 317.20 | 192.20 |
| 3’0” x 6’8” | | 3’2-5/8” x 6’11” | 157.70 | 238.90 | 289.70 | 319.10 | 194.10 |
| 3’0” x 7’0” | | 3’2-5/8” x 7’3” |  | 239.20 |  |  |  |
|  | | | | | | | | |
| lineart-double-door.gif  Includes weather-stripped T-astragal | **Style B – Double** | | | FJBH | SBH | 514SBH | 6916SBH | 6916FJBH |
| **Door Size** | | **Rough Opening** | **4-9/16”**  **Fingerjoint** | **4-9/16”**  **Solid** | **5-1/4”**  **Solid** | **6-9/16”**  **Solid** | **6-9/16”**  **Fingerjoint** |
| 5’0” x 6’8” | | 5’3-3/8” x 6’11”\* | 329.80 | 427.20 | 492.70 | 534.90 | 384.90 |
| 5’4” x 6’8” | | 5’7-3/8” x 6’11”\* | 329.80 | 427.20 | 492.70 | 534.90 | 384.90 |
| 6’0” x 6’8” | | 6’3-3/8” x 6’11”\* | 329.80 | 427.20 | 492.70 | 534.90 | 384.90 |
|  | | | | | | | | |
| lineart-door-single-sidelite.gif | **Style C - 1 Sidelight** | | | 1FJ | 1S | 1514S | 16916S | 16916FJ |
| **Door Size** | | **Rough Opening** | **4-9/16”**  **Fingerjoint** | **4-9/16”**  **Solid** | **5-1/4”**  **Solid** | **6-9/16”**  **Solid** | **6-9/16”**  **Fingerjoint** |
| 3’0” x 6’8” | | 4’4-1/4” x 6’11”\*\* | 354.70 | 499.00 | 567.70 | 646.40 | 414.40 |
|  | | | **Frame is same price with 10”, 12”, or 14” sidelight** | | | | |
| Specify sidelight Left or Right, from the outside looking in  (.SLLJ - SDLT Lock Jamb, .SLHJ - SDLT Hinge Jamb) | | | | | | | |
|  |  | | | | | | | |
| lineart-door-sidelites.gif | **Style D – 2 Sidelights** | | | 2FJ | 2S | 2514S | 26916S | 26916FJ |
| **Door Size** | **Rough Opening** | | **4-9/16”**  **Fingerjoint** | **4-9/16”**  **Solid** | **5-1/4”**  **Solid** | **6-9/16”**  **Solid** | **6-9/16”**  **Fingerjoint** |
| 3’0” x 6’8” | 5’5-3/4” x 6’11”\*\* | | 494.00 | 696.80 | 824.10 | 913.90 | 575.40 |
|  | | | **Frame is same price with 10”, 12”, or 14” sidelights** | | | | |

|  |
| --- |
| \*Rough opening includes weather-stripped T-astragal with flush bolts  🡪For a plain T-astragal, deduct 3/8” from rough opening width  \*\*Rough opening includes 12” sidelights  🡪For each 10” sidelight, deduct 2” from rough opening width  🡪For each 14” sidelight, add 2” to rough opening width |

EDU/DEDU

**Door Unit Options**

***See Page A1 for Standard Specifications, Handing, and Unit Pricing information***

|  |  |  |  |
| --- | --- | --- | --- |
| **Extension Jambs (built up)** | | | |
| **For this jamb** | **Add to this Standard Unit** | **Singles\*** | **Doubles** |
| 9-5/8” FJ Jamb | 4-9/16” FJ Jamb | 96.90 | 121.00 |
| 9-5/8” Solid Jamb | 6-9/16” Solid Jamb | 55.00 | 56.20 |
| 14” Solid Jamb | 6-9/16” Solid Jamb | 111.20 | 123.00 |
| Intermediate size – rip charge (RDJE) | | 10.00 | 10.00 |
| **\***Add an additional ‘Singles’ charge for each installed sidelight or transom | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Additions to Standard Door Unit** | | **Singles** | **Doubles** |
| **Alternate Trim** | Primed FJ Square Edge Casing 1”x3-1/2” (FJSEC) | 28.90 | 38.60 |
| **Size Options** | Oversize Single Unit 3’0” to 4’0” Wide | 25% to 3’0” | — |
| Cut Down Flush Door Height \*voids warranty\* (CD) | 55.55 | 111.10 |
| Spread Mull, each, up to 6” | 55.55 | 55.55 |
| **Labor/Prep Options** | Deadbolt Bore (DB1, DB2) | 8.00 | 8.00 |
| 2-3/4” Backset (234) | 8.00 | 8.00 |
| Peep Sight Bore (PHOLE) | 8.00 | 8.00 |
| Hang Customer’s Door \*subject to approval\* | 100.00 | 200.00 |
| **Sill Options** | Outswing (includes NRP hinge) | 8.75 | 28.90 |
| Bronze Oak Adjustable | 22.70 | 44.90 |
| Aluminum Oak Adjustable | 10.70 | 22.00 |
| Long Sill Horns | 28.00 | 28.00 |
| **Hinge Options** | 4”x4” Solid Brass (3SBHE, 3SBHEBH) | 50.00 | 100.00 |
| 4”x4” Bright Brass Plated (3BBHE, 3BBHEBH) | 6.00 | 12.00 |
| 4”x4” #26D Dull Chrome (326DHE, 326DHEBH) | 6.00 | 12.00 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Deductions From Standard Door Unit** | | **Singles** | **Doubles** |
| **Standard Unit Less:** | Threshold Sill (NSS, NDS) | (24.00) | (46.50) |
| Weatherstrip (NWS, NWSBH) | (4.00) | (6.20) |
| FJ Brick Moulding (NFJB) | (21.70) | (26.00) |
| Solid Brick Moulding (NSB) | (44.30) | (53.10) |
| Weather-stripped T-astragal (NT) | — | (85.90) |

|  |  |
| --- | --- |
| Other Components | |
| Exterior Wood Doors | Section B |
| Sidelights | Page A4 |
| Transoms | Page A5 |
| Multipoint Locks | Page A6 |

|  |  |  |  |
| --- | --- | --- | --- |
| 1701.jpg | 1702.jpg | 1703.jpg | 1705.jpg |
| **1 Light** | **1 Light**  **1 Raised Panel** | **3 Light**  **1 Raised Panel** | **5 Light** |

HSL/HTR

**Pine Sidelights**

|  |  |  |  |
| --- | --- | --- | --- |
| **Description** | **Size** | **Item #** | **List** |
| 1 Light IG | 10” x 1-3/8” | 101I\* | 271.16 |
| 1 Light IG | 12” x 1-3/8” | 121I | 275.16 |
| 1 Light IG | 14” x 1-3/8” | 141I\* | 311.02 |
| 1 Light IG / Raised Panel | 10” x 1-3/8” | 101PI | 271.16 |
| 1 Light IG / Raised Panel | 12” x 1-3/8” | 121PI | 275.16 |
| 5 Light IG True Divided Light | 12” x 1-3/8” | 125DVI\* | 275.16 |
| 5 Light Single Glazed | 12” x 1-3/8” | 125T | 195.40 |
| **Pine Grille Bars** |  |  |  |
| Grille Bar with Clips for 10” Sidelight |  | 10BAR | 3.50 |
| Grille Bar with Clips for 12” Sidelight |  | 12BAR8 | 3.50 |

\*non-stock item


DFE/GR

**“Energy Guard” Fir Sidelights**

|  |  |  |  |
| --- | --- | --- | --- |
| **Description** | **Size** | **Item #** | **List** |
| 1 Light IG (9-3/4” Bottom Rail) | 12” x 1-3/4” | EG4701 | 285.94 |
| 1 Light IG / Raised Panel | 12” x 1-3/4” | EG4702 | 303.92 |
| 3 Light IG True Divided Light / Raised Panel | 12” x 1-3/4” | EG4703 | 319.00 |
| 5 Light IG True Divided Light | 12” x 1-3/4” | EG4705 | 341.04 |
| **Full Surround Fir Grilles** |  |  |  |
| 3 Light Grille for 1 LT/RP (EG4702) |  | GB103 | 37.08 |
| 5 Light Grille for 1 LT (EG4701) |  | GB105 | 46.92 |

HTR

**1-3/8” Pine Transom Glazed with 7/16” Insulated Glass**



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | | **10” Height** | | **12” Height** | | **12” Height GBG** | |
| **Door Size** | **Sash Width** | **Item #** | **List** | **Item #** | **List** | **Item #** | **List** |
| **2’8”** | 32” | 3210 | 87.16 | 3212 | 87.16 | 3212 GBG | 98.00 |
| **3’0”** | 36” | 3610 | 93.90 | 3612 | 93.90 | 3612 GBG | 104.74 |
| **4’0”** | 48” | Special | Please call | 4812 | 113.68 | Special | Please call |
| **5’0”** | 60-1/2” | 6010 | 156.78 | 6012 | 156.78 | 6012 GBG | 172.66 |
| **1’0”/3’0”/1’0”** | 63-1/2” | 6310 | 157.74 | 6312 | 157.74 | 6312 GBG | 177.74 |
| **5’4”** | 64-1/2” | 6410 | 157.74 | N/A | — | N/A | — |
| **1’2”/3’0”/1’2”** | 67-1/2” | Special | Please call | 6712 | 157.74 | 6712 GBG | 189.00 |
| **6’0”** | 72-1/2” | 7210 | 181.36 | 7212 | 181.36 | 7212 GBG | 203.40 |
| **6’0” HPD** | 73-1/2” | 7310 | 181.36 | Special | Please call | N/A | — |
| **Grille Bars** | |  |  |  |  |  |  |
| 10” division bar (5-7/8” O.A.) | | | 10BAR | 3.50 |  |  |  |
| 12” division bar (8” O.A.) | | | 12BAR8 | 3.50 |  |  |  |

**Transom Sash Installed in a Unit**

**Add Sash Price and Framing Charge to Standard Unit List**

|  |  |
| --- | --- |
| **Framing Charge** | |
| 4-9/16” FJ Jamb | 135.30 |
| 4-9/16” Solid Jamb | 212.10 |
| 6-9/16” FJ Jamb | 167.10 |
| 6-9/16” Solid Jamb | 295.80 |

HAR




|  |  |  |  |
| --- | --- | --- | --- |
| **Description** | **Item #** |  | **List** |
| Construction Handle | CHANDLE |  | 16.58 |
| Latch Assembly 6’8” Height | MPLS68LATCH |  | 259.76 |
| Latch Assembly 8’0” Height | MPLS80LATCH |  | 294.94 |
| Lock Trim Regency LH Brushed Nickel | MPLSTRIMLHBN |  | 278.68 |
| Lock Trim Regency RH Brushed Nickel | MPLSTRIMRHBN |  | 278.68 |
| Lock Trim Regency LH Oil Rubbed Bronze | MPLSTRIMLHORB |  | 278.68 |
| Lock Trim Regency RH Oil Rubbed Bronze | MPLSTRIMRHORB |  | 278.68 |

JBEX

**Exterior Door Frames - Knocked Down**

5/4” Rabbeted Jambs ● 1-1/4 x 2” Brick Moulding ● No Sill

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Door Size** | **4-9/16” Solid** | **4-9/16” FJ** | **5-1/4” Solid** | **6-9/16” Solid** | **6-9/16” FJ** |
| **2’8” x 6’8”** | 149.60  (28458SSET) | 70.80  (28458FJSET) | — | — | — |
| **3’0” x 6’8”** | 149.60  (30458SSET) | 70.80  (30458FJSET) | 188.40  (30514SSET) | 211.60  (306916SSET) | — |
| **3’0” x 7’0”** | 151.96  (307456SSET) | — | — | — | — |
| **6’8” Side Jambs Only** | 82.20/pair | 36.90/pair | — | 136.10/pair | 56.90/pair |



**T-Astragals**

|  |  |  |  |
| --- | --- | --- | --- |
| **Size** | **Description** | **Item #** | **List** |
| 6’8”, 1-3/4” | Weather-stripped w/ Flush Bolts | 68TAEQ | 89.76 |
| 7’0”, 1-3/4” | Weather-stripped w/ Flush Bolts | 70TAEQ | 91.34 |

|  |  |  |
| --- | --- | --- |
| **Compression Weatherstrip Set** | Single Door | 7.00 |
| Double Door | 10.50 |

|  |  |  |
| --- | --- | --- |
| **Vinyl Door Sweep (4 fin, brown)** | 2’8” Width | 4.90 |
| 3’0” Width | 4.90 |

JBEX

**Aluminum Threshold Sills**


● 4-5/8” with 2” horns

● Thermal Break

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Inswing - Adjustable**  Oak Riser | | **Inswing - Fixed** | | **Outswing - Fixed** | |
| **Size** | **Item #** | **List** | **Item #** | **List** | **Item #** | **List** |
| 2’8” (32-3/16”) | 32OAKADJ | 32.10 | 32A112 | 22.32 | 321600458 | 30.70 |
| 3’0” (36-3/16”) | 36OAKADJ | 34.02 | 36A112 | 23.64 | 361600458 | 32.82 |
| 6’0” (73-1/8”) | 72OAKADJ | 66.58 | 72A112 | 46.06 | 721600458 | 74.56 |
| 2” Extender for 3’0” |  |  | EE36 | 10.20 |  |  |
| 2” Extender for 6’0” |  |  | A112C | 23.34 |  |  |

SILLPAN

**Door Sill Pans**



|  |  |
| --- | --- |
| **Less 5% on full cartons** | |
| 2’8” & 3’0” | 20 per carton |
| All others | 10 per carton |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | **4-9/16” Jamb** | | **6-9/16” Jamb** | |
| **Size** | **Unit** | **Item #** | **List** | **Item #** | **List** |
| **33-3/4”** | 2’8” Single | SP33754 | 15.92 | SP33756 | 19.80 |
| **37-3/4”** | 3’0” Single | SP37754 | 17.20 | SP37756 | 21.38 |
| **50-1/4”** | 4’0” Bihung | SP5025C4 | 19.42 | SP5025C6 | 24.28 |
| **62-1/4”** | 5’0” Bihung | SP62254 | 20.54 |  |  |
| **66-1/4”** | 5’4” Bihung | SP66254 | 21.10 | SP66256 | 27.94 |
| **74-1/4”** | 6’0” Bihung | SP74254 | 22.94 | SP74256 | 29.24 |
| **63-1/4”** | 5’0” Patio | SP6325C4 | 22.16 |  |  |
| **64-3/4”** | 1’0”/3’0”/1’0” | SP6475C4 | 22.16 | SP6475C6 | 29.34 |
| **72”** | Adjustable  w/ sealant | SPADJ4 | 47.48 | SPADJ6 | 58.34 |

NOVA

**Imagine Series**

DP 50 Sliding Door

5-7/8” Frame Width - can be installed in 4-9/16” or 6-9/16” wall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Size** | **Screen**  **Type** | **Clear**  **w/ Low-E** | **15 Light GBG**  **w/ Low-E** | **Clear**  **w/ Tilt Blinds** | **Clear w/ Raise-**  **Lower Blinds** |
| **5’0” x 6’8”** | Sliding | 1683.46 | 1785.46 | 1,617.92\* | 2025.16 |
| **5’0” x 6’8”** | Retractable | 1780.36 | 1882.46 | — | — |
| **6’0” x 6’8”** | Sliding | 1775.26 | 1877.26 | — | 2116.96 |
| **6’0” x 6’8”** | Retractable | 1872.16 | 1974.16 | — | — |

\*Discontinued - subject to inventory on hand

|  |  |
| --- | --- |
| http://www.ducana.com/images/novatech-imagine-size-1.jpg | http://www.ducana.com/images/novatech-imagine-size-2.jpg |
| OF = Operating left  Fixed right  (XO) | FO = Fixed left  Operating right  (OX) |
|  |  |
| **Rough Opening** | **Overall Dimensions** |
| 5’0” x 6’8” | 59-1/4” x 79-1/2” |
| 6’0” x 6’8” | 71-1/4” x 79-1/2” |

DP 50 single and double swinging patio doors are also available, by special order

|  |
| --- |
| QUANTITY DISCOUNTS FOR SAME SIZE AND KIND DROP SHIPMENT  5 DOORS LESS 5%  10 DOORS LESS 8%  For larger quantities or mixed quantities call for quote |

SHOWROOM DISPLAYS AVAILABLE

Free after purchase of 10 doors